GRAPHIC FILES GUIDE

Please follow these guidelines when submitting your project’s artworks: 

LAYOUT FILES:
· PDF (PDF files are the preferred format for artworks. Please include the bleed area and save without template lines);
· Adobe InDesign (.indd – CS4 – 2019 versions. Please create the package with all fonts and linked images, or export to hi-res PDF without template lines);
· Adobe Illustrator (Please export to hi-res PDF or EPS without template lines);
· Adobe Photoshop (Please export to hi-res PDF without template lines);
· QuarkXPress (Please export to hi-res PDF without template lines)

PHOTOS OR IMAGES:
· PDF (.pdf)
· Photoshop (up to CS5.5 version) (.psd)
· TIFF (.tif)
· Photoshop EPS (.eps)
· JPEG (.jpg)

FONTS:
We accept PostScript, OpenType, or TrueType fonts.
· When providing the file’s package, please include all fonts used for your project.
RESOLUTION:
· All files must have a minimum resolution of 300 dpi (dots per inch). We gladly accept higher resolutions as well.
· Please avoid any image taken from the Internet. They are usually only 72 dpi and are not suitable for printing.

COLOR MODE:
· All files/images must be provided in CMYK color mode (cyan, magenta, yellow, black). (300dpi)
· Please provide all black and white files/images in greyscale color mode. (1200dpi)

BLEED:
The outer edge of the artwork is considered the “safety (or bleed) area” used for cutting. No important images or text should be placed within this area. Although 1/8 of an inch (0.125”) would the minimum size, we strongly recommend using ¼ of an inch (0.25”).  This is all provided in our templates, which can be download here. (qui si apre la pagina dei template)

SAFETY AREA:
During the finishing process there might be a slight displacement. Please keep all critical elements at least 1/8 of an inch (0.125”) from the final cut line (finished edge). We therefore suggest you allowing 1/4 of an inch (0.25”) for bleed.

VINYL LABEL ARTWORKS:
· Please submit all label’s artworks as a solid image, without central holes.
· All previously mentioned color and resolution standards apply to vinyl labels as well.
· Pantone colors are needed as reference for solid color inks on the vinyl’s label.
· All our different templates have guidelines showing its corresponding printing area. You can download here all vinyl label’s printing templates.
· 
DELIVERY:
You can send your artwork files via email to INFO@PPMITALY.COM. 



